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2N® IP SAFETY
ROBUST IP-PORTTELEFON FÖR NÖDSITUATIONER

2N® IP Safety är en förstklassig säkerhetsporttelefon som är utformad för nödkommunikation. Oavsett om den dränks av regn eller utsätts för 
-40°C frost förblir den fullt funktionsduglig och låter dig nå hjälp på en gång och dess ljusa orange färg gör den lätt att hitta i dålig sikt.
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· Robust metallhölje
· Snabb hjälp vid nödsituationer
· Hög uppfattbarhet
· Automatisk test av ljusslinga
· Integration i ditt befintliga system
VARIANTER
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2 knappar - Info och SOS, 10W högtalare

9152102W

1 knapp, 10W högtalare
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Röd nödknapp, 10W 
högtalare
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TECHNICAL PARAMETERS


	Signalling protocol
	
	Mechanical properties
	

	SIP 2.0 (RFC - 3261)
	
	Cover
	Robust aluminium cast product

	
	
	Operating temperature
	−40 °C to 55 °C

	Button
	
	Storage temperature
	−40 °C to 70 °C

	Button design
	Metal buttons with blue backlight or a red emergency button
	Operating relative humidity
	

	
	
	
	10 % – 95 % (non-condensing)

	Number of buttons
	1 or 2
	Dimensions
	217 x 109 x 83 mm

	Numeric keypad
	No
	
	242 x 136 x 83 mm incl. frame

	
	
	Weight
	netto max. 2 kg / brutto max. 2,5 kg

	Audio
	
	Coverage level
	IP69K and IK10

	Microphone
	2 integrated microphones
	

	Amplifier
	10 W (class D)
	

	Loudspeaker
	10 W
	

	Sound pressure level (SPL max)
	
94 dB (10 W type, for 1 kHz, distance 1 m)
	

	Volume control
	Adjustable with automatic adaptive mode
	

	Full duplex
	Yes (AEC)
	

	Audio stream
	
	

	Protocols
	RTP / RTSP
	

	Codecs
	G.711, G.729, G.722, L16/16 kHz
	

	Interfaces
	
	

	Power supply
	PoE or 12V / 2A DC
	

	PoE
	802.3af (Class 0 - 12.95W)
	

	LAN
	10/100BASE-TX s Auto-MDIX, RJ-45
	

	Recommended cabling
	Cat-5e or higher
	

	Supported protocols
	SIP2.0, DHCP opt. 66, SMTP, 802.1x, RTSP, RTP, TFTP, HTTP, HTTPS, Syslog, ONVIF
	

	Passive switch
	NO/NC contacts,
up to 30 V / 1 A AC/DC
	

	Active switch output
	9 up to 13 V DC depending on power supply (PoE: 9 V; adaptor: power supply voltage minus 1 V),
max 600 mA
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